Monitor on OLED display

Transmit data on STM32F4 board

Extract data from Received CAN frame

Is data available in Buffer?

Start